Menu="x-settings"
Title="Interface ethX"
Png="ethernet.png"
---
<?PHP
/* Copyright 2005-2016, Lime Technology
 * Copyright 2012-2016, Bergware International.
 *
 * This program is free software; you can redistribute it and/or
 * modify it under the terms of the GNU General Public License version 2,
 * as published by the Free Software Foundation.
 *
 * The above copyright notice and this permission notice shall be included in
 * all copies or substantial portions of the Software.
 */
?>
<?
// get bond membership
$bond_ethX = $eth0['BONDING']=='yes' ? in_array('ethX',explode(',',$eth0['BONDNICS'])) : false;

// get bridge membership
$bridge_ethX = $eth0['BRIDGING']=='yes' ? in_array('ethX',explode(',',$eth0['BRNICS'])) : false;

$locked = $bond_ethX || $bridge_ethX ;

// get VLAN interfaces
$vlan_ethX = [0];
if (!$locked && isset($ethX)) foreach ($ethX as $key => $val) if (substr($key,0,6)=='VLANID') $vlan_ethX[] = substr($key,7);

$cmd = 'Down';
if (!exec("ip link show ethX|grep -om1 'UP>'")) {
  $more = true;
  $reason = "Interface is shutdown (inactive)";
  $class = 'blue';
  $cmd = 'Up';
} elseif ($bond_ethX) {
  $more = true;
  $reason = "Interface is member of ".$eth0['BONDNAME']." (see interface eth0)";
  $class = 'green';
} elseif ($bridge_ethX) {
  $more = true;
  $reason = "Interface is member of ".$eth0['BRNAME']." (see interface eth0)";
  $class = 'green';
} elseif (empty($ethX)) {
  $more = true;
  $reason = "Interface is not configured";
  $class = 'red';
} else {
  $more = false;
}
?>
<script>
<?if ($tabbed):?>
  var waitid = '#wait_eth0';
<?else:?>
  var waitid = '#wait_ethX';
<?endif;?>
function portcheck_ethX() {
  $.post('/webGui/include/CheckPort.php',{port:'ethX'},function(text) {
    var html = $('#user-notice').html();
    if (!html || html.indexOf('ethX')>0) showNotice(text);
    setTimeout(portcheck_ethX,10000);
  });
}
$(function() {
  var form = document.ethX_settings;
  checkNetworkAccess(form,'ethX');
  checkNetworkSettings(form);
<?if (!$tabbed):?>
  $('div[id=title]').each(function(){
    if ($(this).text().indexOf('Interface ethX')==0) $(this).append("<span id='wait_ethX' class='status red' style='display:none;font-size:small;font-style:italic'>Please wait... configuring interfaces</span>");
  });
<?endif;?>
<?if ($locked || $service):?>
  disableForm(form,true);
<?endif;?>
<?if ($no_eth0):?>
  $('input[name="#shut_ethX"]').prop('disabled',true);
<?endif;?>
  setTimeout(portcheck_ethX,Number('ethX'.substr(3))*1000);
});
</script>
<form markdown="1" name="ethX_settings" method="POST" action="/update.php" target="progressFrame" onchange="exitCode(this,false)" onsubmit="return prepareSettings(this)">
<input type="hidden" name="#file" value="<?=$ini?>">
<input type="hidden" name="#include" value="/webGui/include/update.ethernet.php">
<input type="hidden" name="#section" value="ethX">
<input type="hidden" name="#command" value="/webGui/scripts/netconfig">
<input type="hidden" name="#arg[1]" value="">
<input type="hidden" name="BRNAME" value="">
<input type="hidden" name="BRNICS" value="ethX">
<input type="hidden" name="BRSTP" value="no">
<input type="hidden" name="BRFD" value="0">
<?foreach ($vlan_ethX as $i):?>
<div id="index-ethX-<?=$i?>" markdown="1">
<?if ($i==0):?>
MAC address:
: <?if ($more):?><span class="<?=$class?>"><?endif;?><?=strtoupper(exec("ip link show ethX|grep -Pom1 'ether \K\S+'"))?><?if ($more):?> - <?=$reason?></span><?endif;?>

> This is the hardware address of the interface.
> When tagging is enabled all VLANs on this interface will share the same hardware address.

<?if (!$locked):?>
Enable bridging:
: <select name="BRIDGING" size="1">
  <?=mk_option($ethX['BRIDGING'], "no", "No");?>
  <?=mk_option($ethX['BRIDGING'], "yes", "Yes");?>
  </select>

> Bridging is a feature which creates a virtual bridge and allows VMs to communicate directly with the physical Ethernet port.

<?endif;?>
Interface description:
: <input type="text" name="DESCRIPTION:<?=$i?>" maxlength="40" value="<?=htmlspecialchars($ethX["DESCRIPTION:$i"])?>" onchange="exitCode(this.form,true)">

> Use this field to give addditional information about the purpose of the connection.

IP address assignment:
: <select name="USE_DHCP:<?=$i?>" size="1" onchange="checkNetworkSettings(this.form,<?=$i?>)">
  <?=mk_option($ethX["USE_DHCP:$i"], 'yes', 'Automatic');?>
  <?=mk_option($ethX["USE_DHCP:$i"], 'no', 'Static');?>
  <?=mk_option($ethX["USE_DHCP:$i"], '', 'None');?>
  </select>

> The following settings are possible:
>
> *Automatic* - the server will attempt to obtain its IP address from the local DHCP server<br>
> *Static* - the IP address is manually set for this interface<br>
> *None* - no IP address is assigned to the interface

IP address:
: <input type="text" name="IPADDR:<?=$i?>" maxlength="40" value="<?=$ethX["IPADDR:$i"]?>" class="narrow" pattern="<?=$validIP?>" title="IP address A.B.C.D">

> Greyed out when using DHCP server. Otherwise specify here the IP address of the interface.

Network mask:
: <select name="NETMASK:<?=$i?>" size="1">
  <?=mk_option($ethX["NETMASK:$i"], "255.255.0.0", "255.255.0.0");?>
  <?=mk_option($ethX["NETMASK:$i"], "255.255.252.0", "255.255.252.0");?>
  <?=mk_option($ethX["NETMASK:$i"], "255.255.254.0", "255.255.254.0");?>
  <?=mk_option($ethX["NETMASK:$i"], "255.255.255.0", "255.255.255.0");?>
  <?=mk_option($ethX["NETMASK:$i"], "255.255.255.128", "255.255.255.128");?>
  <?=mk_option($ethX["NETMASK:$i"], "255.255.255.192", "255.255.255.192");?>
  <?=mk_option($ethX["NETMASK:$i"], "255.255.255.224", "255.255.255.224");?>
  <?=mk_option($ethX["NETMASK:$i"], "255.255.255.240", "255.255.255.240");?>
  <?=mk_option($ethX["NETMASK:$i"], "255.255.255.248", "255.255.255.248");?>
  <?=mk_option($ethX["NETMASK:$i"], "255.255.255.252", "255.255.255.252");?>
  </select>

> Greyed out when using DHCP server. Otherwise specify here the associated network mask, by default 255.255.255.0 is selected.

Desired MTU:
: <input type="number" name="MTU" min="68" max="9198" value="<?=$locked?$eth0['MTU']:$ethX['MTU']?>" class="narrow">

> This is the MTU size to use on the physical Ethernet interface.
> If left blank, the MTU will automatically be determined (by default 1500 bytes).

Enable VLANs:
: <select name="TYPE" size="1" onchange="checkNetworkAccess(this.form,'ethX')">
  <?=mk_option($ethX['TYPE'], 'access', 'No');?>
  <?=mk_option($ethX['TYPE'], 'trunk', 'Yes');?>
  </select>
  <span class="pin access-ethX" title="Add VLAN" style="display:none" onclick="addVLAN('ethX',<?=$service?'true':'false'?>)"><i class="fa fa-plus-circle green"></i><em>press to add VLAN</em></span>
<?else:?>
<div class="access-ethX shade-<?=$display['theme']?>" style="display:none" markdown="1">
VLAN number:
: <input type="number" name="VLANID:<?=$i?>" min="1" max="4095" value="<?=$ethX["VLANID:$i"]?>" class="narrow" required>
  <span class="pin" title="Remove VLAN" onclick="removeVLAN($('#index-ethX-<?=$i?>'),<?=$service?'true':'false'?>)"><i class="fa fa-minus-circle red"></i><em>press to remove VLAN</em></span>

> Give each VLAN a unique identifier. Numbers range from 1 to 4095.

Interface description:
: <input type="text" name="DESCRIPTION:<?=$i?>" maxlength="40" value="<?=htmlspecialchars($ethX["DESCRIPTION:$i"])?>" onchange="exitCode(this.form,true)">

> Use this field to give addditional information about the purpose of the connection.

IP address assignment:
: <select name="USE_DHCP:<?=$i?>" size="1" onchange="checkNetworkSettings(this.form,<?=$i?>)">
  <?=mk_option($ethX["USE_DHCP:$i"], 'yes', 'Automatic');?>
  <?=mk_option($ethX["USE_DHCP:$i"], 'no', 'Static');?>
  <?=mk_option($ethX["USE_DHCP:$i"], '', 'None');?>
  </select>

> The following settings are possible:
>
> *Automatic* - the server will attempt to obtain its IP address from the local DHCP server<br>
> *Static* - the IP address is manually set for this interface<br>
> *None* - no IP address is assigned to the interface

IP address:
: <input type="text" name="IPADDR:<?=$i?>" maxlength="40" value="<?=$ethX["IPADDR:$i"]?>" class="narrow" pattern="<?=$validIP?>" title="IP address A.B.C.D">

> Greyed out when using DHCP server or NONE assignment. Otherwise specify here the IP address of the interface.

Network mask:
: <select name="NETMASK:<?=$i?>" size="1">
  <?=mk_option($ethX["NETMASK:$i"], "255.255.0.0", "255.255.0.0");?>
  <?=mk_option($ethX["NETMASK:$i"], "255.255.252.0", "255.255.252.0");?>
  <?=mk_option($ethX["NETMASK:$i"], "255.255.254.0", "255.255.254.0");?>
  <?=mk_option($ethX["NETMASK:$i"], "255.255.255.0", "255.255.255.0");?>
  <?=mk_option($ethX["NETMASK:$i"], "255.255.255.128", "255.255.255.128");?>
  <?=mk_option($ethX["NETMASK:$i"], "255.255.255.192", "255.255.255.192");?>
  <?=mk_option($ethX["NETMASK:$i"], "255.255.255.224", "255.255.255.224");?>
  <?=mk_option($ethX["NETMASK:$i"], "255.255.255.240", "255.255.255.240");?>
  <?=mk_option($ethX["NETMASK:$i"], "255.255.255.248", "255.255.255.248");?>
  <?=mk_option($ethX["NETMASK:$i"], "255.255.255.252", "255.255.255.252");?>
  </select>

> Greyed out when using DHCP server or NONE assignment. Otherwise specify here the associated network mask, by default 255.255.255.0 is selected.

</div>
<?endif;?>
</div>
<?endforeach;?>

<script type="text/html" id="network-template-ethX" markdown="1">
<div id="index-ethX-INDEX" class="access-ethX shade-<?=$display['theme']?>" markdown="1">
VLAN number:
: <input type="number" name="VLANID:INDEX" min="1" max="4095" value="<?=$ethX["VLANID:INDEX"]?>" class="narrow" required>
  <span class="pin" title="Remove VLAN" onclick="removeVLAN($('#index-ethX-INDEX'),false)"><i class="fa fa-minus-circle red"></i><em>press to remove VLAN</em></span>

> Give each VLAN a unique identifier. Numbers range from 1 to 4095.

Interface description:
: <input type="text" name="DESCRIPTION:INDEX" maxlength="40" value="<?=htmlspecialchars($ethX["DESCRIPTION:INDEX"])?>" onchange="exitCode(this.form,true)">

> Use this field to give addditional information about the purpose of the connection.

IP address assignment:
: <select name="USE_DHCP:INDEX" size="1" onchange="checkNetworkSettings(this.form,INDEX)">
  <?=mk_option($ethX["USE_DHCP:INDEX"], 'yes', 'Automatic');?>
  <?=mk_option($ethX["USE_DHCP:INDEX"], 'no', 'Static');?>
  <?=mk_option($ethX["USE_DHCP:INDEX"], '', 'None');?>
  </select>

> The following settings are possible:
>
> *Automatic* - the server will attempt to obtain its IP address from the local DHCP server<br>
> *Static* - the IP address is manually set for this interface<br>
> *None* - no IP address is assigned to the interface

IP address:
: <input type="text" name="IPADDR:INDEX" maxlength="40" value="<?=$ethX["IPADDR:INDEX"]?>" class="narrow" pattern="<?=$validIP?>" title="IP address A.B.C.D">

> Greyed out when using DHCP server or NONE assignment. Otherwise specify here the IP address of the interface.

Network mask:
: <select name="NETMASK:INDEX" size="1">
  <?=mk_option($ethX["NETMASK:INDEX"], "255.255.0.0", "255.255.0.0");?>
  <?=mk_option($ethX["NETMASK:INDEX"], "255.255.252.0", "255.255.252.0");?>
  <?=mk_option($ethX["NETMASK:INDEX"], "255.255.254.0", "255.255.254.0");?>
  <?=mk_option($ethX["NETMASK:INDEX"], "255.255.255.0", "255.255.255.0");?>
  <?=mk_option($ethX["NETMASK:INDEX"], "255.255.255.128", "255.255.255.128");?>
  <?=mk_option($ethX["NETMASK:INDEX"], "255.255.255.192", "255.255.255.192");?>
  <?=mk_option($ethX["NETMASK:INDEX"], "255.255.255.224", "255.255.255.224");?>
  <?=mk_option($ethX["NETMASK:INDEX"], "255.255.255.240", "255.255.255.240");?>
  <?=mk_option($ethX["NETMASK:INDEX"], "255.255.255.248", "255.255.255.248");?>
  <?=mk_option($ethX["NETMASK:INDEX"], "255.255.255.252", "255.255.255.252");?>
  </select>

> Greyed out when using DHCP server or NONE assignment. Otherwise specify here the associated network mask, by default 255.255.255.0 is selected.

</div>
</script>

&nbsp;
: <input type="submit" value="Apply" onclick="$(waitid).show()"><input type="button" value="Done" onclick="done()"><input type="button" name="#shut_ethX" value="Port <?=$cmd?>" onclick="portToggle('ethX','<?=$cmd?>')"><?=$service ? "$service must be <span class='strong big'>Stopped</span> to change (see Settings)" : ""?>
</form>
