Menu="Main:3"
Title="Boot Device"
---
<?PHP
/* Copyright 2005-2016, Lime Technology
 * Copyright 2012-2016, Bergware International.
 *
 * This program is free software; you can redistribute it and/or
 * modify it under the terms of the GNU General Public License version 2,
 * as published by the Free Software Foundation.
 *
 * The above copyright notice and this permission notice shall be included in
 * all copies or substantial portions of the Software.
 */
?>
<script>
function boot_status() {
  var diskio = $.cookie('diskio')===undefined ? 0 : 1;
  $.post('/webGui/include/DeviceList.php',{path:'<?=$path?>',device:'flash'<?if ($tabbed):?>,diskio:diskio<?endif?>},function(data) {
    if (data) {$('#boot_device').html(data); display_diskio();}
<?if ($update && $var['fsState']=='Started'):?>
<?if ($tabbed):?>
    if ($('#tab3').is(':checked')) timer = setTimeout(boot_status,<?=abs($display['refresh'])?>);
<?else:?>
    setTimeout(boot_status,<?=abs($display['refresh'])?>);
<?endif;?>
<?endif;?>
  });
}
<?if ($update && $var['fsState']=='Started' && $tabbed):?>
$('#tab3').bind({click:function() {clearTimeout(timer); boot_status(); $('i.toggle').show('slow');}});
<?else:?>
$('#tab3').bind({click:function() {$('i.toggle').show('slow');}});
<?endif;?>

boot_status();
</script>

<table class="disk_status <?=($var['fsState']=='Stopped'?'small':$display['view']).' '.$display['align']?>">
<thead><tr><td>Device</td><td>Identification</td><td>Temp.</td><td>Reads</td><td>Writes</td><td>Errors</td><td>FS</td><td>Size</td><td>Used</td><td>Free</td><td>View</td></tr></thead>
<tbody id="boot_device">
<?if (isset($disks['flash'])) echo "<tr><td colspan='11'>&nbsp;</td></tr>";?>
</tbody>
</table>

> Vital array configuration is maintained on the USB Flash device; for this reason, it must remain
> plugged in to your server.  Click on [Flash](/Main/Flash?name=flash) to see the GUID and registration
> information, and to configure export settings.  Since the USB Flash device is formatted using FAT file system,
> it may only be exported using SMB protocol.
